SC comment;

If possible, please refer to the table of contents below.

This is an example of Table of Contents for Annex 1-1.4

Annex1-1.4 Technical Description SCADA and SCADA Secure Edition System Overview

1 Introduction

2 SCADA System Offerings

2.1 SCADA Compact; “In-WTG SCADA System”

2.2 SCADA Standard; “Standard SCADA System”

2.3 SCADA Plus; “Enhanced SCADA System”

2.4 Summary of System Functions

3 System Description

3.1 Overview

3.2 SCADA Standard and SCADA Plus System Overview

3.3 Environmental

4 Secure Edition

4.1 Anti-Virus

4.2 Firewall at point of Mingyang data connection

4.4 Switch Hardening

4.5 Secure Mode

4.6 Active Directory

4.7 Domain Controller

4.8 Backup Domain Controller

4.9 Certificate Authority

4.10 Log File Management

4.11 SCADA Secure Edition Product Variants

5 Wind Plant Fiber Optic Network

5.1 Responsibilities

5.2 Single Mode Fiber Optic Cable Specification

5.3 Wind Farm Cable Distance Design Requirements

5.4 Windfarm Network Fiber Loops

6 System Compatibility

7 System Interfaces

7.1 Modbus TCP/IP Client Interfaces to Customer Supplied Metmast Dataloggers

※TCP/IP ：Transmission Control Protocol/Internet Protocol

7.2 Modbus TCP/IP Client Interface to Customer Supplied devices within the Substation

7.3 Customer Integrated IO

※IO：Input / Output

7.4 OPC

※OPC：Open Platform Communications, (formerly “OLE for Process Control”)

8 SCADA Telemetry Testing

9 Customer Input Timeline